**B.PRO COOK Multi-Element**

**BC ME**

**Dimensions:**

Length: 400 mm

Width: 620 mm

Height: 240 mm

**Housing design:**

The multi-element made of CNS 18/10, Material No. 1.4301. with a micro-polished surface consists of a double-walled housing closed on 3 sides with height-adjustable rotating feet.

A cut-out with the dimensions L x W 512 x 305 mm is located on the upper side, acceptance of maximum: GN 1/1.

A cut-out with the dimensions W x H: 332 x 111 mm is located on the operator side, acceptance of maximum: GN 1/1.

The multi-element can be cleaned in a dishwasher.

**Capacity:**

* Top: Hooking in of a GN container with a maximum size of GN 1/1-150 (depending on depth of container at bottom)
* Bottom: Sliding in of a GN container with a maximum size of GN 1/1-100

**Accessories/options:**

* B.PRO GN containers made of CNS or polycarbonate in various sizes and depths, as well as various GN support bars.

**Technical data:**

Material: CNS 18/10, Material No.

Weight: Approx. 7 kg

**Special features:**

* Micro-polished CNS surface
* Large number of loading options with various GN containers

**Make:**

Manufacturer: B.PRO

Model: BC ME

Order No.: 573 458