**B.PRO COOK bain-marie**

**BC BM 700**

**Dimensions:**

Length: 620 mm

Width: 400 mm

Height: 240 mm

**Housing design:**

The bain-marie is made completely of micro-polished stainless steel (AISI 304), equipped with height-adjustable rotating feet. The seamlessly deep-drawn heat retaining wells with large corner radii in 1/1 GN format is made of corrosion-resistant V4A steel (1.4404).

Tray capacity: 1/1 GN-150 or subdivision. The basin features an etched marking that corresponds to the filling amount of approx. 4 litres. On the front of the basin, there is a round drain opening. The drain opening is covered with a lockable safety drain valve.

An operating area, angled towards the rear for improved viewing and operator ergonomics, is seamlessly installed on the front panel to hold the temperature control. The unit is designed to ensure that it can be positioned against a directly adjacent rear wall.

**Electrical equipment:**

The bottom of the basin is heated by a tubular heating element on the underside. Continuous temperature adjustment is carried out with a rotary knob installed in the operating area. 2 indicator lights provide information on the operating mode and heating phase. The unit is completely electrically wired and equipped with a 1.5 m connection cable with a 230 V Schuko plug which exits at a downward angle on the underside.

**Accessories/options:**

* Clamping bar for bridging the gap to other B.PRO COOK units

Order No.: 574 298

**Technical data:**

Material: Stainles steel (AISI 304)

Weight: approx. 15.5 kg

Protection type: IP X4

Heat emission sensitive: 0.09 kW

Heat emission latent: 0.14 kW

Connected load: 230 V / 1N PE AC

50-60 Hz / 0.70 kW

**Special features:**

* Basin made of V4A steel (1.4404)
* Deep basin for GN 1/1-150
* Micro-polished surface made of stainless steel
* Angled operating area

**Make:**

Manufacturer: B.PRO

Type: BC BM 700

Order No.: 574 212